Instructions for MultyVision ISIO software update
=================================================

The MultyVision ISIO instruction manual is available to download
in PDF format for Acrobat Reader at:
http://www.technisat.com 


Installation:
First, copy the following files to a directory of your choice
(e.g. C:\Technisat)


tsdxxxxxxxxxxx.pad
INFO.TXT
autoupdate
singleupdate


USB update instructions
====================

To update the device via the USB interface, you will need a
standard USB flash stick.
Format this USB stick using the FAT32 file system.
Then copy the "tsdxxxxxxxxxxx.pad" file to the stick.


If you only want to run a single update, copy the
"singleupdate" file to the USB flash stick now as well.
If you want to run multiple updates with this USB flash stick, copy the "autoupdate"
file to the USB flash stick instead.

Caution!
You should not have multiple PAD software files located on the flash stick.
Likewise the "autoupdate" and "singleupdate" files should not both be located on the USB flash stick at the same time.


Now switch the device on and insert the USB flash stick into the device's USB
port. After a few seconds a message saying "A USB device has been detected" will appear
on the screen, followed by "Download software from the USB data storage medium". 
The screen will then switch off, and after a few more seconds a message saying
"Updating software. Please wait." will appear, along with
three progress bars that will indicate the progress of the software download
process, the overall progress of the update and the progress of the individual
steps of the update.
The TV picture will then reappear. The TV can now be switched to standby
and the USB flash stick removed.

If the USB update does not start, please repeat all the steps or
try using another USB stick.



(c) TechniSat 2011
Subject to change
