Instructions for software update 
=====================================================

The instruction manual is available to download
in PDF format for Acrobat Reader at:
http://www.technisat.com 


Installation:
First, copy the following files to a directory of your choice
(e.g. C:\Technisat)


xxxxxxxxx.wpad
INFO_EN.TXT
autoupdate
singleupdate


USB update instructions
====================

To update the device via the USB interface, you will need a
standard USB flash stick.
Format this USB stick using the FAT32 file system.
Then copy the "xxxxxxxx.wpad" file to the stick.


If you only want to run a single update, copy the
"singleupdate" file to the USB flash stick now as well.
If you want to run multiple updates with this USB flash stick, copy the "autoupdate"
file to the USB flash stick instead.

Caution!
You should not have multiple PPAD software files located on the USB flash stick.
Likewise the "autoupdate" and "singleupdate" files should not both be located on 
the USB flash stick at the same time.


Now switch the receiver to stand-by and insert the USB stick into the receiver's USB
port. You can now switch the receiver on. After a few
seconds a message saying "Software Update" will appear in the display plus other status updates
as the update is being carried out.
When "Update finished" or "Welcome" appears on the display, the update has finished and
you can remove the stick again.

If the USB update does not start, please repeat all the steps or
try using another USB stick.



(c) TechniSat 2011
Subject to change