Instructions for updating the software on the Nordmende TV Wegavision UHD
=========================================================================

The instruction manual for the Nordmende Wegavision UHD is available to download as a PDF for the
Acrobat Reader at: https://www.nordmende-ce.de/en 


Installation:
=============

Start by copying the "WEGAVISION_UHD_43_4138.zip" ZIP file to a directory of your choice, e.g. C:\Nordmende,
and unzip it to access the contents: 

Folder 3.1.4-4183 with softwarefile "allupgrade_6586.bin"
Info_EN.txt
Info_DE.txt


Important information:
======================

- Please Note: Only install the Software 3.1.4-4183 only on devices with Software 3.1.2-3976k an above. If you use a older Software
  please use the downloadfile WEGAVISION_UHD_43.zip that you can also find on the Nordmende Homepage.

- The update files for the different TV sizes are not compatible with each other, so for example:
  you may only install the files from the "WEGAVISION_UHD_43.zip" Zip file for the "Wegavision UHD 43".
  You may damage the TV otherwise.



USB update instructions
=======================

To update the TV via the USB interface, you will need a standard USB flash memory stick. Format this USB
memory stick with the FAT32 file system.

Update 
- Copy the "allupgrade_6586.bin" software file from the "3.1.4-4183" folder to the USB memory stick.
- Switch on the TV and unplug it while the screen is on (do not switch it off!).
- Insert the USB flash memory stick into the USB port on the TV.
- Now plug the TV back in.
  After a few seconds a blue screen is displayed with a progress indicator showing 0% to 100% while the update
  is in progress.
  When "Software Upgrade complete" (progress bar at 100%) is displayed on the screen, the update is complete.
- Unplug the TV and remove the USB memory stick.
- Wait a few seconds and plug the TV back in.


If the USB update does not start, please repeat all the steps or try using a different USB memory stick.



(c) Nordmende 2019
Subject to change
